##### SUNHANS eSunRC 4000mW 5.8Ghz 36dBm WiFi Signal Booster

*Features:*  
    Excitingly small! Only 59g!  
    5-16V wide voltage range;  
    5.8GHz, Max. 4000mW output power;  
    Aluminum-alloy case by CNC, anti-interference;  
    Full kit, easy to install; light weight,  small size, protable;  
    Designed for Drones, UAV, RC equipment....  
**♦ TX only, Only transmit the signal** **, turn off the receive the signal, the drone remote control terminal can get clearer video and image.**

Product Description:

1. **[Simply plug and play]**

Extend the range of your wireless network with the Indoor Wifi Booster Amplifier.  
Plug and play connections,no software, no configuration and virtually no setup of software.

1. **[Compatible with any 5.8G wireless device],used for transmit need (TX Only).**

Our product can support 5.8G Hz WLAN 802.11a,802.11n,802.11ac,5.8G Hz wireless AP, 5.8G Hz wireless bridge,5.8GHz wireless router, 5.8GHz wireless network card, 5.8GHz wireless monitoring(NVR,DVR), 5.8GHz wireless microphone, 5.8GHz bluetooth,RC drones,FPV device etc

1. **[Maximum Output power].**

The max output power can be up to 4000mW.  
This amplfier will boost the transmit (TX Only) power of your wireless device a whopping 36dBm.